**AI-DRIVEN DYNAMIC FUZZ TESTING FOR IoT SECURITY: DETECTION AND MITIGATION OF DDoS ATTACKS USING GRAPH NEURAL NETWORKS**

A PROJECT REPORT

#### Submitted by

Charvi Jain [RA2111047010113]

#### Under the Guidance of

## Dr. Nagendra Prabhu S.

(Assistant Professor, Department of Computational Intelligence)

### *in partial fulfillment of the requirements* *for the degree of*

## BACHELOR OF TECHNOLOGY

## in

## ARTIFICIAL INTELLIGENCE



## DEPARTMENT OF COMPUTATIONAL INTELLIGENCE

## COLLEGE OF ENGINEERING AND TECHNOLOGY

SRM INSTITUTE OF SCIENCE AND TECHNOLOGY

## KATTANKULATHUR- 603 203

### OCT 2024

Department of Computational Intelligence

##### SRM Institute of Science & Technology

##### Own Work\* Declaration Form

This sheet must be filled in (each box ticked to show that the condition has been met). It must be signed and dated along with your student registration number and included with all assignments you submit – work will not be marked unless this is done.

To be completed by the student for all assessments

##### Degree/ Course : B.Tech Artificial Intelligence, B.Tech Computer Science w/s IoT

**Student Name :** Charvi Jain, Shaurya Singh Srinet, Shounak Chandra

##### Registration Number : RA2111047010113. RA2111032010006, RA2111032010026

**Title of Work :** AI-Driven Dynamic Fuzz Testing for IoT Security: Detection and Mitigation of DDoS Attacks using Graph Neural Networks

We hereby certify that this assessment compiles with the University’s Rules and Regulations relating to Academic misconduct and plagiarism\*\*, as listed in the University Website, Regulations, and the Education Committee guidelines.

We confirm that all the work contained in this assessment is our own except where indicated, and that We have met the following conditions:

* Clearly referenced / listed all sources as appropriate
* Referenced and put in inverted commas all quoted text (from books, web, etc)
* Given the sources of all pictures, data etc. that are not my own
* Not made any use of the report(s) or essay(s) of any other student(s) either past or present
* Acknowledged in appropriate places any help that we have received from others (e.g. fellow students, technicians, statisticians, external sources)
* Compiled with any other plagiarism criteria specified in the Course handbook / University website

We understand that any false claim for this work will be penalized in accordance with the University policies and regulations.

|  |
| --- |
| **DECLARATION:** |
| We are aware of and understand the University’s policy on academic misconduct and plagiarism, and we certify that this assessment is our own work, except where properly referenced, and that we have followed the good academic practices outlined above. |
| If you are working in a group, please write your registration numbers and sign with the date for every student in your group. |

**ACKNOWLEDGEMENT**

We express our humble gratitude to **Dr. C. Muthamizhchelvan,** Vice-Chancellor, SRM Institute of Science and Technology, for the facilities extended for the project work and his continued support.

We extend our sincere thanks to Dean-CET, SRM Institute of Science and Technology,   
**Dr. T.V. Gopal,** for his invaluable support.

We wish to thank **Dr. Revathi Venkataraman,** Professor & Chairperson, School of Computing, SRM Institute of Science and Technology, for her support throughout the project work.

We are incredibly grateful to our Head of the Department, **Dr. R. Annie Uthra**, Professor and Head, Department of Computational Intelligence, School of Computing, SRM Institute of Science and Technology, for her suggestions and encouragement at all the stages of the project work.

We want to convey our thanks to our Project Coordinator, **Dr. M. S. Abirami**, Associate Professor, Panel Head, **Dr. M Uma**, Associate Professor, Department of Computational Intelligence, School of Computing, SRM Institute of Science and Technology, for their inputs during the project reviews and support.

We register our immeasurable thanks to our Faculty Advisor, **Dr. E Poongothai,** Department of Computational Intelligence, School of Computing, SRM Institute of Science and Technology, for leading and helping us to complete our course.

Our inexpressible respect and thanks to our guide**, Dr. Nagendra Prabhu S,** Assistant Professor, Department of Computational Intelligence, SRM Institute of Science and Technology, for providing us with an opportunity to pursue our project under his mentorship. He provided us with the freedom and support to explore the research topics of our interest. His passion for solving problems and making a difference in the world has always been inspiring.

We sincerely thank the Computational Intelligence Department staff and students, SRM Institute of Science and Technology, for their help during our project. Finally, we would like to thank parents, family members, and friends for their unconditional love, constant support, and encouragement.

Shaurya Singh Srinet [RA2111032010006]

Shounak Chandra [RA2111032010026]

Charvi Jain [RA2111047010113]



# SRM INSTITUTE OF SCIENCE AND TECHNOLOGY KATTANKULATHUR – 603 203

## BONAFIDE CERTIFICATE

Certified that 18CSP107L project report titled **“AI-Driven Dynamic Fuzz Testing for IoT Security: Detection and Mitigation of DDoS Attacks Using Graph Neural Networks”** is the bonafide work of “**SHAURYA SINGH SRINET [RA2111032010006], SHOUNAK CHANDRA [RA2111032010026], CHARVI JAIN [RA2111047010113]”** who carried out the project work under my supervision. Certified further, that to the best of my knowledge the work reported herein does not form any other project report or dissertation based on which a degree or award was conferred on an earlier occasion on this or any other candidate.

|  |  |  |  |
| --- | --- | --- | --- |
| **DR. NAGENDRA PRABHU S.** | | **DR. R. ANNIE UTHRA** | |
| **ASSISTANT PROFESSOR** | | **HEAD OF THE DEPARTMENT** | |
| DEPARTMENT OF COMPUTATIONAL INTELLIGENCE | | DEPARTMENT OF COMPUTATIONAL INTELLIGENCE | |
|  | |  | |

##### 

Examiner I Examiner II

**TABLE OF CONTENTS**

[**ABSTRACT**](#_bookmark1) **v**

[**LIST OF FIGURES**](#_bookmark2) **vi**

[**LIST OF TABLES**](#_bookmark2) **vii**

[**ABBREVIATIONS**](#_bookmark3) **viii**

[**1 INTRODUCTION**](#_bookmark4) **1**

* 1. The Emerging Threat of DDoS Attacks for IoT Networks 1
  2. Impact of Real-time Detection and Mitigation 1
  3. Dynamic Fuzz Testing Framework with AI 1
  4. Contribution and Future Prospects 2

[**2 LITERATURE SURVEY**](#_bookmark20) **3**

2.1 IoT Security Challenges 3

2.2 DDoS Attacks on IoT Networks 3

2.3 AI-Based IoT Security Solutions 4

2.4 Dynamic Fuzz Testing for IoT Security 5

2.5 NS3 Simulations for IoT Security 5

**3** [**SYSTEM A**](#_bookmark30)**RCHITECTURE AND DESIGN 7**

3.1 Layered Architecture Overview 7

3.1.1 Device Layer 7

3.1.2 Security and Detection Layer 7

3.1.3 Fuzz Testing Layer 7

3.1.4 Mitigation Layer 8

3.1.5 Edge Computing and Analytics Layer 8

3.1.6 Cloud Processing Layer 8

3.2 Core Components of FuzzAIoT 8

3.2.1 Graph Neural Networks (GNNs) 8

3.2.2 Fuzz Testing Engine 9

3.2.3 Traffic Filtering Module 9

3.2.4 Mitigation Engine 9

3.3 Scalability and Performance Considerations 9

3.3.1 Scalability 9

3.3.2 Low Latency Operations 9

3.3.3 Adaptability 10

3.4 Integration with Existing Infrastructure 10

3.4.1 Cloud and Edge Integration 10

3.4.2 Legacy System Compatibility 10

3.5 Summary of System Design 10

**4 METHODOLOGY 11**

4.1 Addressing IoT Security using AI-Driven Techniques 11

4.2 Dynamic Fuzz Testing 11

4.2.1 Introduction to Dynamic Fuzz Testing 11

4.2.2 Data Generation through Fuzz Testing 13

4.3 Dataset Preprocessing 13

4.3.1 XML to CSV from Simulation Data 13

4.3.2 Data Labelling and Balancing 13

4.4 Training AI Model 14

4.4.1 Model Architecture 14

4.4.2 Training Process and Hyperparameter Tuning 15

4.4.3 Validation 15

4.5 Simulation Environment 15

4.5.1 Network Setup 15

4.5.2 Traffic Simulation 16

4.5.3 Visualization with NetAnim 16

4.6 Mitigation Strategy 16

4.6.1 Blocking of malicious IPs 16

4.6.2 Evaluation and Refinement 16

**5 CODING AND TESTING 17**

5.1 Simulation Setup in NS3 17

5.1.1 Network Topology Design 17

5.1.2 Traffic Generation 18

5.1.3 Mobility Model 20

5.1.4 Setting up NetAnim 21

5.2 Dataset Generation 21

5.2.1 Traffic Data Collection 21

5.2.2 Data Conversion into CSV Format 21

5.2.3 Data Balancing 24

5.3 AI Model Training 25

5.3.1 Model Architecture 25

5.3.2 Training Process 27

5.3.3 Validation 27

5.4 Mitigation in NS3 – Real Time detection and Action 28

5.4.1 Detection of Malicious IP Address 28

5.4.2 Packet Filtering 28

5.5 Conclusion of Testing and Implementation 29

**6 RESULTS AND DISCUSSIONS 30**

6.1 Introduction 30

6.2 Results 30

6.2.1 Training and Accuracy of the GNN Model 30

6.2.2 Results of Validation 31

6.2.2.1 Validation Accuracy 31

6.2.2.2 Confusion Matrix 31

6.2.3 Mitigation Strategy 32

6.2.3.1 Packet Dropping 32

6.2.3.2 Performance on Network 32

6.3 Visualization of Results 32

6.3.1 Loss and Accuracy Graphs 33

6.3.2 Confusion Matrix 34

6.3.3 Network Animation 35

**7 CONCLUSION AND FUTURE ENHANCEMENT 36**

7.1 Summary of Headings 36

7.1.1 AI-Driven Dynamic Fuzz Testing 36  
 7.1.2 NS3 Simulation and Visualization 37

7.1.3 Counter Measures 37

7.2 Future Improvements 37

7.2.1 Real-Time Mitigation 38

7.2.2 Elaborated Attack Scenarios 38

7.2.3 Scalability Test 38

7.2.4 Adaptive Learning 39

7.2.5 Integration of Security Tool 39

7.3 Conclusion 39

**REFERENCES 41**

**APPENDIX**

**A CONFERENCE PUBLICATION 44**

**B PLAGIARISM REPORT 45**

**ABSTRACT**

The exponential growth in IoT adoptions has brought such networks to be much more vulnerable to Distributed Denial of Service attacks. In the DDoS attack, network performance issues and device vulnerabilities are exploited for inflicting far-reaching disruptions. Traditional IoT security solutions have proven inadequate in detecting and mitigating sophisticated threats in a timely and efficient manner, leaving IoT systems exposed to serious risks. This paper therefore presents an AI-driven security framework to adapt the detection and mitigation approach of DDoS attacks in IoT networks through dynamic fuzz testing and its integration into Graph Neural Networks (GNNs). This approach enables real-time identification and neutralization of malicious activities. The framework leverages the NS3 simulation tool to create realistic and diversified network traffic flows, which are used to train the GNN model. As a result, the model is prepared to handle various traffic patterns and attack scenarios, making it robust against real-world conditions. Once deployed in a live environment, the model monitors network traffic, identifies DDoS attacks, and mitigates them without disrupting legitimate IoT operations. The proposed framework achieved a 74% detection accuracy and a 95% success rate in mitigation during trials, highlighting its scalability and adaptability. This capability ensures that the framework can effectively address present and future IoT security challenges. The integration of AI with dynamic fuzz testing offers comprehensive protection, ensuring the integrity, availability, and reliability of IoT networks, making it an essential component of future IoT architectures by providing high-quality security against evolving DDoS threats.

v

**LIST OF FIGURES**

3.1 Architecture Layers . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8

##### [4.1 Architecture Model](#_bookmark12) . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12

[4.2 GNN Architecture Model](#_bookmark16) . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14

6.1 GNN Model Training Accuracy Graph . . . . . . . . . . . . . . . . . . . . . 33

6.2 GNN Model Training Loss Graph . . . . . . . . . . . . . . . . . . . . . . . 33

6.3 Class Distribution Graph . . . . . . . . . . . . . . . . . . . . . . . . . . . . 34

6.4 Confusion Matrix . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 34

6.5 Network Animation Simulation . . . . . . . . . . . . . . . . . . . . . . . . . 35

vi

**ABBREVIATIONS**

**IoT** Internet of Things

**AI** Artificial Intelligence **GNN** Graph Neural Networks

**DDoS** Distributed Denial of Service

**NS3** Network Simulator 3

**SYN Flood** Synchronize Flood

**XML**  Extensible Markup Language

**CSV** Comma-Separated Values **IP** Internet Protocol

**SMOTE** Synthetic Minority Oversampling Technique

**GCN** Graph Convolution Network

**TCP** Transmission Control Protocol

**UDP** User Datagram Protocol

**NetAnim** Network Animator

**IDS** Intrusion Detection System

**SIEM** Security Information and Event Management

vii

**CHAPTER 1**

**INTRODUCTION**

* 1. **The Emerging Threat of DDoS Attacks for IoT Networks**

The quick expansion of the Internet of Things (IoT) linking devices to enhance efficiency also leads to heightened vulnerabilities. Perhaps one of the most critical challenges rising with increasing vulnerability is the DDoS attack. In a DDoS attack, compromised devices-often called bots-sent malicious traffic to overflow the targeted network, breaking its normal operations.

IoT devices are most prone to such attacks due to very low computing capabilities and weak security features. Once such devices come into the hands of attackers, it becomes a tool of immense DDoS attack through botnet and services go totally down with the likelihood of data breaches and financial loss.

* 1. **Impact of Real-time Detection and Mitigation**

Traditional solutions of IoT security fail to detect most of the DDoS attacks, especially in real time. Most IoT devices tend to be extremely interconnected, with highly dynamic network traffic flows; hence, any type of proactive measure for security should be able to identify and neutralize such threats at the moment they may arise.

Minimizing damage due to DDoS attacks requires real-time detection and mitigation. Malicious traffic overload servers unless acted on in real time, hence resulting in system downtime and decreased performance. This poses the need for highly sophisticated security frameworks that can respond quickly to threats under IoT settings if perpetual service availability is to be sustained.

* 1. **Dynamic Fuzz Testing Framework with AI**

The framework identifies the limitation that currently exists with IoT security approaches and proposes an AI-driven Dynamic Fuzz Testing framework that incorporates GNNs as a sophisticated solution for real-time DDoS detection and mitigation. Analyzing network traffic patterns, the GNN-based model differentiates between legitimate and malicious traffic, thereby enabling dynamic and accurate threat response capabilities.

1

It is based on simulations with NS3. Simulations are based on real traffic data and, by virtue of normal and attack conditions, are used in training the model to identify a vast number of attacks. Thus, the robustness in the detection capability is realized. It integrates the model into an IoT network through which continuous monitoring of traffic at the entry points can be done. Malicious sources are identified and blocked without affecting legitimate operations.

* 1. **Contribution and Future Prospects**

The Dynamic Fuzz Testing framework offers several key contributions to IoT security, which also comprises state-of-the-art DDoS mitigation approaches. First, this approach, in contrast to the traditional methods, poses an AI-driven approach for real-time DDoS detection and mitigation. It uses GNN in such a way that complex patterns and relationships within traffic can be learned by the model, thereby making it more accurate and efficient towards threat detection.

One of the most interesting facts this project demonstrates is the framework's ability to handle high traffic loads, even in complex network topologies, with no loss in overall performance.

The future for the project is to concentrate on improving real-time capabilities within the system, including expanding its scope in attacking scenarios it may address, and adaptive learning to meet emerging threats. The framework can also be used in conjunction with other security tools to develop an all-rounded defense system against IoT networks offering stronger protection against evolving cyber-attacks.

**1.5 Sustainable Development Goal of the Project**

**1.5.1 IoT Security for Strong Resilient Infrastructure**

IoT has been penetrating all the nooks and corners of the world, and so, it needs to be made safe in the form of DDoS attacks in the context of cyber-attacks. Internet of Things devices are now in use in a number of large sectors that run from health to transport and from agricultural activities to energy. All of these falls under modern operations; hence, any slight failure in security terms would threaten the number of elements working and therefore challenge critical information and relevant services in highly precious scenarios.

Relating to our project, we are designing AI-based dynamic fuzz testing with GNN and dynamic packet filtering for tracking, prevention, and therefore mitigation of cyber-attacks on an IoT network. This can, therefore be said in terms of the strategy of fuzz testing probing vulnerabilities in IoT systems dynamically to create adaptive and robust solutions for the protection of IoT against DDoS attacks and other types of security attacks that service downtimes will be averted with possible data breaches, cascading failures that would be resultant from such an attack causing chaos in the critical infrastructure which may, in a way, serve as contributing to sustainable development.

As AI-driven fuzz testing protects these devices, it safeguards the heart of what the world's critical infrastructure means: to keep us moving forward. They make sure that systems for the operation of industry, communities, and government services stand unwavering; thus, they speak for a future safer and more secure, sustainable as the technology has enabled.

With the proliferation of IoT networks in motion, this AI-driven fuzz testing role becomes most imperative to be adopted as it supports resilient infrastructure, which is something that SDG 9 visualizes.

**1.5.2. Industrialization with inclusivity and sustainability**

IoT devices are fully engaged in the automation process as well as in the efficiency process of supply chains and are even available in real time for data availed that can be made to provide decisions across industries. Thus, it increases productivity all wastages are averted, so these industries have been leaner and greener.

The biggest risks associated with such machines are because of cyber-attacks, owing to heavy connectivity through weak inbuilt security features that have been embedded into the device, making the whole network vulnerable to the same.

Our AI-based fuzz testing solution will secure the IoT devices of industries against potential threats that could become serious security breaches. Fuzz testing tests and finds those weak points in devices and in software and communication channels so that the possibility of such cyber incidents that may culminate in a shutdown of total operations is reduced. This will give more confidence to the industries to embrace IoT technology without compromising safety for sustainable and inclusive growth by making sure that IoT integration will be safe and reliable.

This holds much more promising security assurance for developing economies where industrial IoT adoption is growing but likely to be stifled by a dearth of resources in hand to be used for their cybersecurity. That can be due to its AI-based fuzz testing that creates an opportunity to have such economies by offering them economical automated solutions in IoT security since it enables new sustainable developments through new jobs and resource optimization, building the atmosphere in which the advanced technology can be achieved without chaotic growth and prosperity for every nation.

Advancement in Cyber Security and Artificial Intelligence It's the advanced form of cyber security from the traditional methodology. With the power of AI, Fuzz testing can now exhibit dynamic prediction and detection relative to threats, with agile responses to those dangers that would be able to provide intelligence beyond what traditional methodologies can achieve in terms of detecting static applications or rule-based applications found in the traditional security solutions. Graph Neural Networks pave the way to adaptability as well as scalability in that process. That is, the AI models are, therefore capable of hence are able to analyze complex patterns of Internet of Things network traffic to establish possible attacks in its evolution thus providing proactive cybersecurity. It makes it easy to apply latest techniques of AI and, therefore, encourages even more research into areas concerning cybersecurity as well as developing artificial intelligence. Innovation births new tools and methodologies that get implemented in financial systems, health care systems, manufacture and other transportation systems. These investment flows in sustainable technology solutions lead to an economic environment that encourages the establishment of innovation and safety together. In light of such better protection of critical infrastructures, industries can comfortably adopt sophisticated, integrated technologies. With these cyber threats, this evolution of AI-based fuzz testing brings avenues for interdisciplinary cooperation at the same time as these experts in data science, cybersecurity, and integration of network engineering are embraced. Valuable technological innovation and sustainable as well as secure development gets added up because responsible as well as ethical use of AI always precedes development; so its most precious technological asset is well-guarded with it.

2

**CHAPTER 2**

**LITERATURE SURVEY**

**2.1 Challenges in the IoT Security**

IoT devices pose security vulnerabilities due to the heterogeneity of such devices and limited computational ability. This makes IoT networks highly susceptible to DDoS attacks. The principal challenges include the following:

• Device Vulnerabilities: These devices are usually unsecured at the time of their deployment, which tends to expose them to some attack.

• Missing Secure Communication Protocols: Absence of secure communication increases the probability of man-in-the-middle and other interception types of attacks.

• Outdated Firmware: Many IoT devices lack frequent updates, which increases vulnerability.

**2.2 DDoS Attacks in IoT Networks**

DDoS attacks are the main concern since IoT networks have a large scale of flooded services that will disrupt them. The key findings for research are:

• Botnet Attacks: For example, large botnets like Mirai emphasize vulnerabilities within interconnected IoT devices.

• Mitigation Strategies: The current approach is generally based on the traffic monitoring or DDoS-resistant protocols. Since their effectiveness varies due to resource limitations on IoT devices, the following is adopted.

**2.3 AI-Based Security Solutions for IoT**

Artificial Intelligence including machine learning, deep learning, is promising, in order to enhance IoT security, as it can detect any anomalous network behavior, which includes the following:

• Graph Neural Networks (GNNs): GNNs learn about connections within IoT networks and enable a higher DDoS detection precision with spatial data processing.

• Weakness of Traditional Machine Learning Approaches: Current traditional machine learning methods have problems handling IoT network data as they tend to be large in volume and highly complex; the latter, in particular, can be managed more suitably by GNNs.

**2.4 Dynamic Fuzz Testing for IoT Security**

Advanced IoT protocol vulnerability detection, further enhancing resilience to DDoS attacks is offered through dynamic fuzz testing, which involves

• System Stress Testing: Unexpected inputs using fuzz testing identify weak spots that attackers can leverage upon.

• AI-Powered Fuzz Testing: Combination of fuzz testing with GNNs enhances detection and mitigation capabilities to support adaptive security measures.

**2.5 Limitations Identified from Literature Survey (Research Gaps)**

The literature presents several limitations in current IoT security research:

• Real-time Detection is Missing: All of the frameworks lack the detection and response of real-time DDoS attacks, particularly when large IoT networks are considered.

• Adaptive Learning is Rarely Implemented: Adaptive learning is rarely seen to update for the latest emerging threats; therefore, models already developed are old-fashioned due to changes in the strategy of the attackers.

• Underutilization of GNNs in Security: Although GNNs are promising, their usage in complex IoT network interactions may be underutilized for the identification of coordinated attacks.

• Simulation-Based Testing Not Fully Utilized: Limited usage of network simulation tools like NS3 leads to a reduction in the robustness of the model, as these tools may simulate IoT environments and attack scenarios more effectively.

This project aims to bridge the gaps by focusing on the following objectives:

• An IoT DDoS detection and mitigation frame should be designed using an adaptation of GNNs based models for its processing capabilities in real-time

• The security architecture will include adaptive learning features that make the whole frame learn about changes happening in the threat landscapes

• The usage of NS3 in terms of simulation is crucial since an NS3 model allows providing realistic networking scenarios through robust simulations.

• AI-based Dynamic Fuzz Testing For protection against very rare as well as quickly changing patterns of cyber attacks that an IoT system would be under stress to perform, let's apply dynamic fuzz testing on GNNs.

**2.6 Product Backlog (Major User Stories and Expected Outcome)**

A structured set of prioritized user stories intended to keep track of this product's development. What each says of what could be expected out of a feature:

• Network Administrator shall be allowed to run this model and select which traffic was a DDoS hit and which are legitimate moving into the IoT traffic destined to a network in virtually real-time.

• As a security engineer, the model ought to have adaptive learning to help ensure that its detection capability remains relevant as regards different attacking types.

• As a developer, test the model by simulating an IoT environment to its reliability in practice.

**2.6 Project Road Map**

The roadmap of work for the project is made up of major work phases such as:

• Literature Review, Requirement gathering and Analysis of research gaps.

• Phase 2: GNN-based detection integration with dynamic fuzz testing.

• Phase 3: Setup for NS3 simulation testing for realistic validation.

• Phase 4: Testing, validation, and optimization of performance in the simulated environment.

• Phase 5: Documentation and final reporting along with any recommendations for real-world implementation.

6

**CHAPTER 3**

**SYSTEM ARCHITECTURE AND DESIGN**

**3.1 Layered Architecture Overview**

The FuzzAIoT framework is built using a layered approach, where each layer performs distinct tasks related to device security, DDoS detection, and mitigation, as well as machine learning-driven traffic analysis. This modular design ensures scalability, maintainability, and flexibility, allowing for seamless integration and updates without disrupting the entire system.

**3.1.1 Device Layer**

The Device Layer consists of IoT devices that collect and transmit data throughout the network. Because they usually have low computing power, these can be easily exploited when attacking. It uses mechanisms based on encryption and authentication to secure the devices so that only authorized devices can use the network.

**3.1.2 Security and Detection Layer**

This is the core layer where DDoS detection occurs. It uses Graph Neural Networks (GNNs) to analyze traffic patterns and detect anomalies. The GNNs model the communication between IoT devices, allowing the system to identify unusual patterns that indicate a DDoS attack. The layer continuously monitors the network to ensure quick detection of potential threats.

**3.1.3 Fuzz Testing Layer**

The Fuzz Testing Layer performs Dynamic Fuzz Testing on IoT communication protocols to detect vulnerabilities. This layer continuously tests the devices with various inputs to identify weak points in protocol communication, which attackers could exploit. Once a vulnerability is detected, the system either patches it or isolates the affected device to prevent any damage.

7

**3.1.4 Mitigation Layer**

The Mitigation Layer is responsible for neutralizing threats once an attack is detected. It enforces security policies through techniques like traffic filtering, rate limiting, and traffic re-routing to ensure that legitimate traffic continues uninterrupted while blocking malicious traffic. The layer dynamically adapts to new threats and can update mitigation strategies in real-time.


**3.1.5 Edge Computing and Analytics Layer**

This layer distributes processing tasks to edge nodes, reducing latency and providing faster response times during attacks. By performing traffic filtering and initial DDoS detection at the network edge, critical security decisions are made closer to the source of the data, ensuring quick reactions without overloading central servers.

**3.1.6 Cloud Processing Layer**

For more computationally intensive tasks like large-scale traffic analysis and machine learning model training, the Cloud Processing Layer handles these operations. It also stores historical data for long-term analysis, integrates with external systems, and supports more in-depth analytics that improve detection and response to future threats.

Fig. 3.1 Architecture Layers



**3.2 Core Components of FuzzAIoT**

**3.2.1 Graph Neural Networks (GNNs)**

GNNs form the backbone of the FuzzAIoT's real-time traffic analysis and DDoS detection. By modeling IoT devices and their communication as a graph, GNNs can identify unusual traffic patterns or communication anomalies. This graph-based approach enhances the detection accuracy of DDoS attacks by analyzing relationships between network nodes and their communication paths.

8

**3.2.2 Fuzz Testing Engine**

The Fuzz Testing Engine continuously probes IoT communication protocols by generating dynamic inputs to identify potential vulnerabilities. It works closely with the GNNs to flag devices with weak protocols and take necessary measures to mitigate these risks. This engine ensures that devices are regularly tested for weaknesses that could be exploited in a DDoS attack.

**3.2.3 Traffic Filtering Module**

The Traffic Filtering Module employs machine learning algorithms to classify and filter incoming traffic. This component plays a crucial role in distinguishing between legitimate traffic and malicious traffic during a DDoS attack. By ensuring that only safe traffic is allowed through, this module maintains network integrity while preventing overload during an attack.

**3.2.4 Mitigation Engine**

The Mitigation Engine is responsible for implementing strategies that limit the impact of a detected attack. Techniques such as traffic shaping, blacklisting malicious IPs, and re-routing ensure that the attack traffic is minimized without affecting legitimate communications. This engine dynamically adjusts mitigation efforts based on the attack's severity and nature.

**3.3 Scalability and Performance Considerations**

**3.3.1 Scalability**

FuzzAIoT is designed to handle large IoT networks with potentially thousands of devices. The layered architecture and edge computing capabilities enable the system to scale efficiently without degrading performance. The distributed nature of traffic filtering and attack detection across edge nodes and the cloud ensures that the system remains responsive even as the network grows.

**3.3.2 Low Latency Operations**

Latency is very important for real-time responses in IoT networks, particularly for such sectors as healthcare or industrial IoT. FuzzAIoT architecture minimizes latency at the architecture level, pushing the critical traffic analysis and filtering into the Edge Computing Layer. Mitigation thereby happens close to the source of data generation, hence minimizing the latency in attack responses.

9

**3.3.3 Adaptability**

The system’s modular design ensures that new detection and mitigation techniques can be easily integrated. The architecture is adaptable to evolving attack vectors and future IoT technologies, ensuring that the framework remains effective in a rapidly changing threat landscape.

**3.4 Integration with Existing Infrastructure**

**3.4.1 Cloud and Edge Integration**

FuzzAIoT seamlessly integrates with both cloud platforms and edge devices. While the Edge Computing Layer provides real-time threat detection and response, the Cloud Processing Layer handles resource-heavy tasks, ensuring an optimal balance between latency reduction and data processing capabilities.

**3.4.2 Legacy System Compatibility**

The system is designed to integrate with legacy IoT infrastructure, making it suitable for deployment in a wide variety of environments. It supports common protocols and communication standards, ensuring that even older devices can benefit from enhanced security without requiring significant system overhauls.

**3.5 Summary of System Design**

FuzzAIoT’s layered architecture and modular components are built to provide real-time protection against DDoS attacks in IoT networks. The system’s reliance on Dynamic Fuzz Testing and Graph Neural Networks (GNNs) ensures proactive detection and mitigation of attacks while maintaining scalability, low latency, and adaptability for future IoT developments.

By dividing responsibilities across distinct layers—from the Device Layer to the Cloud Processing Layer—the architecture ensures efficient security measures at each stage of the data flow. Additionally, the system’s ability to integrate with existing infrastructure makes it a flexible and robust solution for securing diverse IoT deployments.

10

**CHAPTER 4**

**METHODOLOGY**

**4.1 Addressing IoT Security Using AI-Driven Techniques**

The Internet of Things is an explosively growing domain in which smart home appliances, industrial sensors, and much more can interact and be used independently. Although this is very efficient and widely automated, the large-scale deployment of IoT devices triggers fresh network security concerns. Probably the most relevant threat here is DDoS attacks, where malicious actors try to overwhelm IoT networks with excessive traffic generation.

This project will propose a hybrid strategy combining fuzz testing, AI techniques, and network simulation for DDoS attack detection and mitigation. Here, GNN in fuzzy testing is used as the core for traffic pattern analysis as well as the identification of malicious activity in real-time.


**4.2 Dynamic Fuzz Testing**

**4.2.1 Introduction to Dynamic Fuzz Testing**

Fuzzing, or fuzz testing, is basically a testing technique that injects malformed or unexpected inputs into a system to expose potential weaknesses. Dynamic fuzz testing is a superior instrument that relates to investigating and finding the vulnerabilities in network security when abnormal traffic patterns emerge during DDoS attacks in IoT. Bugs, misconfigurations, and exploitable weaknesses are successfully detected in fuzz testing in real-world-like scenarios.

The project will simulate a wide array of IoT network traffic behaviors—from the simplest normal IoT communication to highly complex malicious DDoS attempts—by injecting unexpected data into the IoT ecosystem. This will bring to the project's attention vulnerabilities that it would otherwise have never known about had it taken the conventional approach to testing. The anomalies in the network traffic thus serve as a means of training AI models on distinct datasets for the improvement of detection capacity in relation to attack patterns.

11



**Fig. 4.1 Architecture Diagram**

12

**4.2.2 Data Generation Through Fuzz Testing**

Data generation based on fuzz testing is important to give a precise representation of normal and malicious traffic. This process involves generating or synthesizing traffic through the help of fuzz testing tools and then configuring them in a manner that simulates potential attack vectors. Thus, the flow of packets generated through such a method brings out the closest imitation of common DDoS attacks, like SYN floods, UDP amplification, or botnet-induced flooding.

The simulation environment is set up to mirror a wide variety of network traffic behaviors. The resulting dataset captures multiple attack vectors, thereby subjecting the AI models that are trained on this data to various patterns. Traffic is labeled to distinguish between benign and malicious activity; thus, it creates a foundation for training machine learning models. Through such a well-balanced dataset, the system can generalize more effectively when detecting real-time attacks.

**4.3 Dataset Preprocessing**

**4.3.1 XML to CSV from Simulation Data**

Realistic IoT Network Simulations through NS3 feed the AI model with relevant data. The raw simulation data is produced in XML format, recording timestamps, source and destination IPs, packet size, etc. Though well-structured, XML isn't a good data source to be fed directly to train machine learning models. This custom script transforms the XML data into a simplified and more machine learning-friendly CSV format.

This step has the added advantage of handling large sets of data using frameworks like TensorFlow or PyTorch, which ensure the integrity of the data being processed. This allows easy manipulation of that data, feature extraction, and preprocessing for easy analysis.

**4.3.2 Data Labeling and Balancing**

Besides, the dataset needs to be properly labeled and balanced. That is the classification between benign traffic and attacks—a step necessary to prevent training a biased model towards one class. Moreover, having a balanced dataset avoids favoring benign or malicious traffic within an AI model, making it more robust to new data.


13

On the labeled dataset, further preprocessing is carried out in normalization of packet size, traffic frequency, and source/destination IP addresses. In case there is class imbalance, other methods like SMOTE (Synthetic Minority Over-sampling Technique) could be used. This way, both benign and attacking traffics are distributed equally in the training dataset.

**4.4 Training AI Model**

It is an AI project with a Graph Neural Network (GNN) as the type of training it does, which is supposed to classify IoT network traffic as being either benign or malicious. It is best for this task because it can consider relationships between nodes—take, for instance, the IoT devices—and learn to pick up complex traffic patterns that are hard to capture using traditional machine learning models.

**4.4.1 Model Architecture**



**Fig. 4.2 GNN Model Architecture**

14

The architecture of the GNN captures spatial and temporal dependencies in the traffic dataset. It accounts for interconnectivity as well as communication between different IoT devices, which are termed nodes. It captures how the patterns within a network change with time. In such a manner, through amalgamation of aspects of both spatial and temporal, GNN traces the path of the traffic flow and identifies anomalies that indicate DDoS attacks.

The architecture design is multi-layered graph convolutional networks (GCNs) that process traffic data and analyze the underlying patterns. One could include attention mechanisms that focus on relevant features in the dataset to make it even better at DDoS attack recognition.

**4.4.2 Training Process and Hyperparameter Tuning**

It performs training of the GNN model in iterations with the labeled dataset. Multiple epochs of training analyze the performance of the model in terms of accuracy, precision, recall, and F1-score. Through the process, hyperparameter tuning of learning rates, batch sizes, and the number of graph convolutional layers has been carried out. Cross-validation techniques are applied in the process of training to ensure the model generalizes well to unseen data. It is the most critical step to avoid overfitting and ensure that the model can pick up attacks or otherwise in a real scenario.

**4.4.3 Validation**

The trained model is then validated on freshly simulated environment traffic data. During the validation process, the model is tested against diverse network configurations, and its capability to detect DDoS attacks is examined in different network setups, thus generalizing well to new unseen data. The results are analyzed to improve the model, if needed, either by adjusting hyperparameters or the architecture.

**4.5 Simulation Environment**

**4.5.1 Network Setup**

The NS3 simulator offers a realistic testbed for the IoT network, which contains different IoT devices that can connect to a server via a central router. This simulation environment further generates both legitimate and malicious traffic, while the latter simulates a DDoS attack launched by bot nodes. The simulation ensures a realistic representation of IoT traffic, which allows the GNN model to learn from authentic traffic patterns.

15

**4.5.2 Traffic Simulation**

The capabilities of NS3's traffic generation capability are used to simulate TCP and UDP flows like real-world network traffic. On-Off traffic generators will simulate attacks such as DDoS, while BulkSend applications simulate normal flows in a network. The captured traffic is for a period and then written to files so that it can be used both to train and test the AI model.

**4.5.3 Visualization with NetAnim**

To further visualize the network behavior, NetAnim has been used by graphing the traffic flow and interaction between IoT devices. From this graphical output, a better view is obtained on the disturbance caused to normal traffic patterns due to DDoS attacks and how mitigating strategies have been designed to work in real-time. This validation is of paramount importance while testing the mitigation mechanisms in the system.

**4.6 Mitigation Strategy**

**4.6.1 Blocking of Malicious IPs**

The heart of the mitigation strategy is the dynamic blocking of identified malicious IP addresses due to the GNN model's detection. Upon identification of an attack, the NS3 simulation environment imposes router-level actions that block packets from such malicious IP addresses and prevent further disruption to the traffic. This packet filtering mechanism ensures that even during attacks, the network remains operational with minimal effects on legitimate traffic.

**4.6.2 Evaluation and Refinement**

The mitigation strategy is evaluated in terms of network performance before and after the introduction of blocking mechanisms. Metrics such as delivery ratio, latency, and throughput are analyzed to assess the effectiveness of the mitigation. Feedback from the simulation executions is used to iteratively refine the strategy so that it can handle a variety of attack scenarios.

16

**CHAPTER 5**

**CODING AND TESTING**

This means the project was taken on around critical milestones that would ensure DDoS attacks on an IoT network are detected and mitigated. Advanced AI techniques, particularly Graph Neural Networks (GNNs), made this testbed: a real-world within an NS3 simulation environment that aimed to improve real-time DDoS detection and mitigation systems using GNN-based models. This chapter details the simulation setup data production, as well as training, integrating the trained AI model in the NS3 environment, which then provides real-time attack identification and mitigation.

**5.1 Simulation Setup in NS3**

The first critical step in the process of testing was modeling the IoT simulation environment in NS3, which indeed could basically mimic real IoT device behaviors and network attack patterns. This simulated benign and malicious traffic pattern was essential in the generation of traffic that would assist in the validation of the ability of the system to detect and mitigate DDoS attacks.

**5.1.1 Network Topology Design**

The network topology design was therefore essential to the success of the project. The network was a natural or typical example of an IoT environment where central routers mediate traffic between a set of IoT devices and a server.

* IoT Devices: The simulation included many IoT devices. Some of them include smart home appliances, like smart speakers, thermostats, and security cameras. In this way, such devices would send benign traffic to the central server as legitimate data packets. In this experiment, a total of 20 IoT devices were simulated to mimic close-to-reality cases.
* Bot Nodes. In the network, 5 bot nodes mimicked a DDoS attack through their malicious traffic. Bot nodes are compromised IoT devices taken over by a botnet. They overwhelm the server due to heavy data traffic.
* Router and Server: In the architecture, the router would be working as a central hub on which benign and malicious traffic flow. All the intensity of DDoS attack fell on the server, with this architecture especially filtering the traffic reaching the server, and that is also with the help of routers.

17

**5.1.2 Traffic Generation**

Realistic traffic patterns accurately represent the behavior of an IoT network.

* Benign Traffic: This was created using the feature of TCP BulkSend, simulating typical data uploads from IoT devices, such as sensor readings or status updates. The benign traffic sent was low volume and periodic. The NS3 pseudocode is as follows:

BEGIN Simulation

DEFINE experimental parameters:

UDP\_PORT = 9001

TCP\_PORT = 9000

TCP\_RATE = "10Gbps"

MAX\_SIMULATION\_TIME = 1200 seconds

SEND\_SIZE = 64 bytes

NUM\_TCP\_CONNECTIONS = 10

INITIALIZE network components:

Create nodes: iotDevices (1 device), router (1 device), server (1 device)

DEFINE Point-To-Point link attributes:

Data Rate = TCP\_RATE

Channel Delay = 0.1 ms

INSTALL network devices:

Connect iotDevices to router and router to server via Point-To-Point links

ASSIGN IP addresses:

Set base IP address for network with specified subnet mask

Assign IP addresses to all devices

CONFIGURE multiple TCP connections between IoT Device and Server:

FOR each TCP connection (up to NUM\_TCP\_CONNECTIONS):

SET bulk send application on IoT device to send unlimited traffic

SET send size to SEND\_SIZE for packet size

INSTALL bulk send application on IoT device

START bulk send application at time 0

STOP bulk send application at MAX\_SIMULATION\_TIME

END FOR

CREATE TCP sinks on Server:

FOR each TCP connection:

CONFIGURE TCP sink application on server to receive packets on specific TCP\_PORT

START TCP sink application at time 0

18

STOP TCP sink application at MAX\_SIMULATION\_TIME

END FOR

POPULATE routing tables

CONFIGURE node mobility and positions for visualization:

SET router, server, and iotDevices to fixed positions

SET layout parameters for network visualization

CREATE animation output file "BenignTraffic.xml" and enable packet metadata

RUN Simulation

END Simulation

* Malicious Traffic: Bot nodes using On-Off traffic generators generated malicious traffic, which produced bursty, high-rate UDP traffic designed to flood the server. The traffic was like that shown in real-world DDoS attacks-traffic spikes, which are hard to predict and overwhelming of the server. The NS3 pseudocode is as follows:

BEGIN DDoS Simulation

DEFINE experimental parameters:

UDP\_SINK\_PORT = 9001

TCP\_SINK\_PORT = 9000

DDOS\_RATE = "100Mbps"

MAX\_SIMULATION\_TIME = 100 seconds

NUMBER\_OF\_BOTS = 5

INITIALIZE network components:

Create nodes: iotDevices (1 legitimate device), router (1 device), server (1 device)

Create botNodes for attack traffic with NUMBER\_OF\_BOTS devices

DEFINE Point-To-Point link attributes:

Data Rate = DDOS\_RATE

Channel Delay = 1 ms

INSTALL network devices:

Connect iotDevices to router and router to server via Point-To-Point links

Connect each botNode to router with individual Point-To-Point links

ASSIGN IP addresses:

Set base IP address for network with specified subnet mask

Assign IP addresses to each bot on a unique subnet

Assign IP addresses to IoT device, router, and server

CONFIGURE DDoS Application on botNodes:

FOR each botNode (up to NUMBER\_OF\_BOTS):

SET OnOff application to UDP traffic with constant rate and on/off times

INSTALL OnOff application on each botNode

19

START OnOff application at time 0

STOP OnOff application at MAX\_SIMULATION\_TIME

END FOR

CONFIGURE legitimate TCP traffic from IoT Device to Server:

SET BulkSend application to TCP traffic with unlimited data size and packet size 1024 bytes

INSTALL BulkSend application on IoT device

START BulkSend application at time 0

STOP BulkSend application at MAX\_SIMULATION\_TIME

SET UDP Sink on Server:

CONFIGURE UDP sink to receive packets on specified UDP\_SINK\_PORT

START UDP Sink application at time 0

STOP UDP Sink application at MAX\_SIMULATION\_TIME

SET TCP Sink on Server:

CONFIGURE TCP sink to receive packets on specified TCP\_SINK\_PORT

START TCP Sink application at time 0

STOP TCP Sink application at MAX\_SIMULATION\_TIME

POPULATE routing tables

CONFIGURE node mobility and positions for visualization:

SET router, server, and botNodes to fixed positions

SET layout parameters for network visualization

CREATE animation output file "DDoSTraffic.xml" and enable packet metadata

RUN Simulation

END Simulation

**5.1.3 Mobility Model**

The Constant-Position-Mobility-Model was utilized to simulate static nodes. Such static IoT devices, like household appliances, as represented by the model, would remain in fixed positions when they were in action. Though static, the system dynamically monitored their traffic patterns with a constant network topology at any point in time.

20

**5.1.4 Setting up NetAnim**

The visualization tool NetAnim was used to allow vivid animation of network traffic and behaviors under normal operation as well as DDoS attack conditions.

* Node Placement: Many nodes were placed around the central router and server at distances where the network interactions are visible. The IoT devices and bot nodes are positioned across from each other.
* Packet Flows and Effect of the Attack: NetAnim was an important thing for visualizing the packet flows and how the nodes interact with one another, as well as the effect caused by the DDoS attacks on the network. Clearly, it differentiated between benign and malicious traffic flows and even extracted insight into the effects of various mitigations.

**5.2 Dataset Generation**

Based on this simulation environment, a dataset containing benign and malicious traffic patterns was generated next. The size of the dataset is what made it crucial in the training of the AI model on how to detect and classify DDoS attacks.

**5.2.1 Traffic Data Collection**

For the simulation, traffic was captured by logging every packet passed to the router. This included benign and malicious traffic. The data logged in an XML file meant that through that format, I was able to capture critical details such as timestamp, source IP, destination IP, and packet size.

**5.2.2 Data Conversion into CSV Format**

For converting the XML logs into a format suitable for training the AI model, custom scripts were used. It has been chosen primarily due to direct compatibility with most of the machine learning frameworks and due to the efficiency of maintaining required network features in an organized manner.

* Feature Extraction: Important features, such as packet size, source/destination IP addresses, and traffic patterns, were extracted from the data for the training purpose.
* Labelling: Each packet of data was labeled as benign or DDoS according to whether it originated from a legitimate IoT device or bot node.

21

* XML to CSV conversion pseudocode for Benign Traffic is as follows:

IMPORT XML parsing and CSV writing libraries

IMPORT regex library for IP and size extraction

DEFINE FUNCTION parse\_benign\_xml\_to\_csv WITH parameters:

- xml\_file: XML input file containing packet data

- csv\_file: output CSV file

- benign\_ip\_prefix: prefix indicating benign traffic sources

BEGIN FUNCTION parse\_benign\_xml\_to\_csv

LOAD XML data from xml\_file

GET root of the XML document

OPEN csv\_file in write mode

INITIALIZE CSV writer and write header row: ["Timestamp", "Source", "Destination", "PacketSize", "Label"]

SET packet\_count = 0 // Total packets processed

SET benign\_count = 0 // Count of benign packets

FOR each packet element in XML root:

GET 'meta-info' attribute of packet

IF 'meta-info' attribute exists THEN:

EXTRACT timestamp from 'fbTx' attribute OR default to '0' if not present

EXTRACT source and destination IP addresses using regex on 'meta-info'

IF IP addresses are found THEN:

EXTRACT packet size using regex on 'meta-info' OR default to '0' if not present

CHECK if source IP starts with benign\_ip\_prefix:

IF TRUE, SET label to "Benign"

WRITE row to CSV with [timestamp, source\_ip, destination\_ip, packet\_size, label]

INCREMENT benign\_count

END IF

INCREMENT packet\_count

END IF

DISPLAY total packets processed and total benign packets

END FUNCTION

22

* XML to CSV conversion pseudocode for DDoS Traffic is as follows:

IMPORT XML parsing and CSV writing libraries

IMPORT regex library for IP and size extraction

DEFINE FUNCTION parse\_ddos\_xml\_to\_csv WITH parameters:

- xml\_file: XML input file containing packet data

- csv\_file: output CSV file

- ddos\_ips: list of IP prefixes identifying DDoS traffic sources

BEGIN FUNCTION parse\_ddos\_xml\_to\_csv

LOAD XML data from xml\_file

GET root of the XML document

OPEN csv\_file in write mode

INITIALIZE CSV writer and write header row: ["Timestamp", "Source", "Destination", "PacketSize", "Label"]

FOR each packet element in XML root:

GET 'meta-info' attribute of packet

IF 'meta-info' attribute exists THEN:

EXTRACT timestamp from 'fbTx' attribute OR default to '0' if not present

EXTRACT source and destination IP addresses using regex on 'meta-info'

IF IP addresses are found THEN:

EXTRACT packet size using regex on 'meta-info' OR default to '0' if not present

CHECK if source IP matches any prefix in ddos\_ips:

IF TRUE, SET label to "DDoS"

ELSE, SET label to "Unknown"

WRITE row to CSV with [timestamp, source\_ip, destination\_ip, packet\_size, label]

END IF

END IF

DISPLAY message indicating successful DDoS traffic export to CSV

END FUNCTION

23

* XML to CSV conversion pseudocode for Validation generation setup is as follows:

IMPORT XML parsing and CSV writing libraries

IMPORT regex library for IP and size extraction

DEFINE FUNCTION parse\_xml\_to\_csv WITH parameters:

- xml\_file: XML input file containing packet data

- csv\_file: output CSV file

- ddos\_ips: list of IP prefixes identifying DDoS traffic sources

- benign\_ips: list of IP prefixes identifying benign traffic sources

BEGIN FUNCTION parse\_xml\_to\_csv

LOAD XML data from xml\_file

GET root of the XML document

INITIALIZE ddos\_count and benign\_count to 0

OPEN csv\_file in write mode

INITIALIZE CSV writer and write header row: ["Timestamp", "Source", "Destination", "PacketSize", "Label"]

FOR each packet element in XML root:

GET 'meta-info' attribute of packet

IF 'meta-info' attribute exists THEN:

EXTRACT timestamp from 'fbTx' attribute OR default to '0' if not present

EXTRACT source and destination IP addresses using regex on 'meta-info'

IF IP addresses are found THEN:

EXTRACT packet size using regex on 'meta-info' OR default to '0' if not present

DETERMINE traffic label based on source IP:

IF source IP matches any prefix in ddos\_ips:

SET label to "DDoS"

INCREMENT ddos\_count

ELSE IF source IP matches any prefix in benign\_ips:

SET label to "Benign"

INCREMENT benign\_count

ELSE:

SKIP packet (no matching IP ranges)

WRITE row to CSV with [timestamp, source\_ip, destination\_ip, packet\_size, label]

END IF

END IF

DISPLAY total DDoS packets, total benign packets, and total packets processed

END FUNCTION

24

* XML to CSV main driver conversion pseudocode for all the three is as follows:

DEFINE FUNCTION main

SET xml\_file to path of the XML file generated by NS-3

SET csv\_file to output path for the CSV file

DEFINE ddos\_ips as a list of IP prefixes associated with DDoS attack sources

DEFINE benign\_ips as a list of IP prefixes associated with benign sources

DISPLAY message indicating the start of XML processing

CALL parse\_xml\_to\_csv FUNCTION with arguments:

- xml\_file

- csv\_file

- ddos\_ips

- benign\_ips

DISPLAY message confirming CSV file has been saved after conversion

END FUNCTION

IF script is run directly THEN

CALL main FUNCTION

END IF

**5.2.3 Data Balancing**

By balancing the dataset provided, which would have otherwise been biased due to an AI model's favor toward one class of data, the modeling aspect was taken care of to prevent biased weightings toward one class of data on the part of the AI model. This ensured that the model had equal numbers of both benign and malicious packets, so it may learn to correctly classify either type of traffic. The pseudocode to balance the dataset is as follows:

IMPORT pandas library for data manipulation

DEFINE FUNCTION combine\_csv\_files WITH parameters:

- benign\_csv: path to the benign traffic CSV file

- ddos\_csv: path to the DDoS traffic CSV file

- output\_csv: path for the combined output CSV file

LOAD benign traffic CSV into benign\_df

LOAD DDoS traffic CSV into ddos\_df

DETERMINE minimum number of rows between benign\_df and ddos\_df

24

SAMPLE both benign\_df and ddos\_df to contain min\_rows rows each, with a fixed random state for consistency

CONCATENATE benign\_df and ddos\_df into a single DataFrame combined\_df

SHUFFLE combined\_df to mix benign and DDoS rows, using a fixed random state

SAVE combined\_df to output\_csv without row indices

DISPLAY message confirming combined CSV file has been saved

END FUNCTION

DEFINE FUNCTION main

SET benign\_csv to path of benign traffic CSV file

SET ddos\_csv to path of DDoS traffic CSV file

SET output\_csv to output path for combined CSV file

CALL combine\_csv\_files FUNCTION with benign\_csv, ddos\_csv, and output\_csv

END FUNCTION

IF script is run directly THEN

CALL main FUNCTION

END IF

**5.3 AI Model Training**

The dataset was then prepared, and training the GNN model on detecting DDoS attacks was the job done.

**5.3.1 Model Architecture**

The GNN model was designed to study the node interactions in the network. It was trained with the classification of traffic as either benign or malicious.

* Input Layer: This was a feed made up of the raw features from the CSV dataset.
* Hidden Layers: These layers took the data streams in and looked for patterns that distinguished benign from DDoS traffic.
* Output Layer: This output layer spewed out the entire classification, whether it was benign or malicious.
* GNN identification pseudocode is as follows:

IMPORT necessary libraries for data processing, neural networks, and visualization

DEFINE GCN MODEL CLASS:

- INIT function:

CREATE two GCNConv layers:

25

1. First layer with input channels 1 and output channels 16

2. Second layer with input channels 16 and output channels 2 (for two classes: Benign, DDoS)

- FORWARD function:

APPLY first convolution layer on data with edge index

APPLY ReLU activation

APPLY second convolution layer

RETURN output

DEFINE FUNCTION load\_data WITH parameter:

- csv\_file: path to the CSV dataset

LOAD CSV data into a pandas DataFrame

EXTRACT PacketSize as node features and Label as target labels

CONVERT PacketSize to tensor of floating-point values

CONVERT Label to tensor of integer values (1 for DDoS, 0 for Benign)

CREATE edge\_index tensor with self-loops for each node

RETURN Data object containing node features, edge index, and labels

DEFINE FUNCTION train\_gnn\_model WITH parameters:

- data: dataset for training

- model: GCN model instance

- epochs: number of training epochs (default 150)

INITIALIZE optimizer with model parameters and learning rate

INITIALIZE loss criterion as cross-entropy loss

SET model to training mode

CREATE lists to store training loss and accuracy for each epoch

FOR each epoch:

ZERO gradients

PERFORM forward pass to get model output

CALCULATE loss and backpropagate

UPDATE model parameters with optimizer

COMPUTE accuracy by comparing predictions to actual labels

STORE loss and accuracy for visualization

DISPLAY epoch number, loss, and accuracy

RETURN trained model, list of losses, and list of accuracies

DEFINE FUNCTION validate\_gnn\_model WITH parameters:

- model: trained GCN model

- validation\_data: dataset for validation

SET model to evaluation mode

PERFORM forward pass to get model output

26

COMPUTE accuracy on validation set

DISPLAY validation accuracy

GENERATE classification report and confusion matrix

DISPLAY confusion matrix as heatmap

DEFINE FUNCTION plot\_training\_metrics WITH parameters:

- losses: list of loss values

- accuracies: list of accuracy values

PLOT training loss over epochs

PLOT training accuracy over epochs

DEFINE FUNCTION main

SET paths to training and validation datasets

LOAD training and validation data

INITIALIZE GCN model

CALL train\_gnn\_model with training data, model, and specified epochs

SAVE trained model to specified path

PLOT training metrics

CALL validate\_gnn\_model with trained model and validation data

IF script is run directly THEN

CALL main FUNCTION

END IF

**5.3.2 Training Process**

This model was trained using this labeled dataset by minimizing errors and increasing accuracy.

* Loss Function: Utilize the loss function to track how much each class predicted was different from the actual class in the data set. With each iteration, it updated the model's parameters so that its errors were minimized.
* Hyperparameter Tunwas In relation to hyperparameters, the learning rate, hidden layers, and the size of the batch were all properly tuned for optimal model performance via iterative training.

**5.3.3 Validation**

After every training epoch, the model was validated on a separate dataset to ensure that it generalized very well to new, unseen data. Techniques for preventing overfitting were also put in place to ensure that the model did not perform well only on training data but could handle real-world scenarios.

27

**5.4 Mitigation in NS3 – Real-time detection and Action**

The final stage involved implementing the trained GNN model in the NS3 simulation environment to facilitate real-time detection and mitigation of DDoS attacks.

**5.4.1 Detection of Malicious IP Address**

The trained GNN was implemented within the NS3 environment through processing real-time network traffic. Each packet's features were analyzed by the algorithm, which asserted the malicious IP addresses involved in the DDoS attack and detected them in real time.

**5.4.2 Packet Filtering**

Once such malicious IP address identities were known, they were placed in a blocklist. A router level packet filtering mechanism prevented the packets from reaching the server by dropping those packets coming from identified malicious IP addresses, reducing the spread of this attack. Pseudocode for Packet Filtering is as follows:

IMPORT necessary NS-3 modules

DEFINE CONSTANTS:

- UDP\_SINK\_PORT, TCP\_SINK\_PORT

- DDOS\_RATE for attack traffic, TCP\_RATE for legitimate traffic

- MAX\_SIMULATION\_TIME

- NUMBER\_OF\_BOTS, NUMBER\_OF\_IOT\_DEVICES

DEFINE FUNCTION GetDeviceFromIp to retrieve device from IP address for packet dropping:

FOR each node in nodes:

CHECK if node has interface with given IP

IF interface exists, RETURN the device associated with the IP

RETURN nullptr if no match found

BEGIN main FUNCTION

PARSE command-line arguments

SET simulation time resolution

ENABLE logging for UDP echo applications

CREATE nodes for IoT devices, router, server, and bot nodes

CONFIGURE Point-To-Point links:

SET data rate and delay attributes

28

INSTALL Point-To-Point connections:

- BETWEEN router and server

- BETWEEN each bot and router

- BETWEEN each IoT device and router

INSTALL Internet stack on all nodes

ASSIGN IP addresses to bot nodes, server, and each IoT device with unique subnets

DEFINE list of malicious IPs (detected by GNN model)

FOR each malicious IP:

FIND device associated with IP

IF device found, SET device callback to drop packets

CONFIGURE DDoS attack behavior:

INITIALIZE OnOff application for each bot node with UDP traffic

SET traffic rate, on-time, and off-time attributes

INSTALL OnOff applications on bot nodes and set start/stop times

CONFIGURE legitimate traffic from IoT devices:

FOR each IoT device:

INITIALIZE BulkSend application with TCP traffic to server

SET unlimited packet transmission with specified packet size

INSTALL BulkSend application on IoT device and set start/stop times

SET UDP Sink application on server to receive UDP packets

SET TCP Sink application on server to receive TCP packets

POPULATE routing tables

CONFIGURE node positions for visualization:

- SET positions for router, server, bot nodes, and IoT devices with specified spacing

CREATE AnimationInterface object for XML output

ENABLE packet metadata in the animation file

SET custom positions for nodes

RUN and DESTROY the simulation

END main FUNCTION

**5.5 Conclusion of Testing and Implementation**

The deployment and testing of this system clearly showed how an AI-driven DDoS mitigation system can detect and mitigate attacks in real-time conditions. Comparing packet delivery ratio, latency, and server loads before and after the attacks being mitigated, the AI-driven system proved to maintain network performance even while under a DDoS attack.

29

**CHAPTER 6**

**RESULTS AND DISCUSSIONS**

**6.1 Introduction**

In modern IoT networks, the growing number of connected devices has increased risks in the DDoS attack concerning security. Most of the devices are characterized as heterogeneous in terms of the mesh of networks through which they are connected; it alone is a rich playground for malicious entities to launch attacks using compromised devices as vectors for widespread damage. This problem is beyond the capabilities of traditional security mechanisms because most IoT devices are resource-constrained, and the attack patterns change dynamically, evolve over time, and make use of space and signature-based techniques.

To address this problem, we created an AI-Driven Dynamic Fuzz Testing approach using GNNs that is tested on the NS3 network simulation to identify and counter DDoS attacks.

**6.2 Results**

As shown clearly in the results below, the approach identifies malicious traffic patterns while using an active mitigation strategy to safeguard IoT systems.

**6.2.1 Training and Accuracy of the GNN Model**

We used the synthetic dataset produced with large NS3 simulations for our training. We included both benign and DDoS traffic to make the model learn from both types of patterns. The class balance of the dataset was ensured before training, making sure that the two types were equal. We show two plots below showing training loss and accuracy:

The training loss, as depicted in the first graph, displays a very sharp dip during the preliminary stages of training. The learning by the model is represented here. At the initial stages, the loss was high because the data was unknown to the GNN. However, training loss declined very sharply down to 0 as epochs proceeded, reflecting that the model correctly identified the patterns from the data. At around 40 epochs, the loss curve stabilizes and becomes around 0, indicating convergence of the model.

30

The second plot is the training accuracy: it oscillates around 50%, which might imply that the model was simply wandering through its features and updating its weights with back-propagation. Accuracy increases steadily with epochs, peaking at a high of 100%, implying that GNN learned to classify the training data with full accuracy. But training with 100% accuracy may overfit; sometimes the model might go very well on the training data but may not generalize well using new unseen data.

**6.2.2 Results of Validation**

While impressive accuracy on the training set, the real strength of the model is in performance over unseen data. We judged the GNN on a validation set extracted from an independent set of simulations using NS3. This validation dataset also contained an equal proportion of benign and DDoS traffic compared to the training data.

**6.2.2.1 Validation Accuracy:**

The average validation accuracy achieved by the GNN model is 74%. While this is quite lower than the corresponding training accuracy, it still indicates that the model learns well from the data. Lower validation accuracy generally means that, in most cases, the model would correctly detect DDoS traffic while normally and effectively responding; however, there are probably some edge cases or variations in the attack patterns that it has not been able to classify correctly. This promises a good level of performance since it will be deployed in real-world scenarios of new evolving types of DDoS attacks.

**6.2.2.2 Confusion Matrix:**

The confusion matrix for the validation results shows even further the model's ability to distinguish between benign and malicious traffic. It presents a relatively healthy scale of true positives, which are the correct identification of DDoS attacks, and true negatives, referring to the correct identification of benign traffic. Moreover, the matrix also indicates false positives and false negatives. In practice, a false positive (major classification of benign traffic as malicious) might prompt unwarranted mitigating steps, whereas a false negative DDoS traffic will not be detected, permitting attacks to run amok. Minimizing these types of errors will, therefore, be critical in increasing the reliability of the system.

31

**6.2.3 Mitigation Strategy**

Detection is only half the equation; mitigation is equally important so that the IoT network stays healthy. The GNN identifies malicious traffic, and then the strategy for packet filtering engages to block packet traffic coming from those malicious IP addresses.

**6.2.3.1 Packet Dropping:**

By using such a model in the NS3 simulation, the malicious IP addresses were easily traced, and their packets dropped. Packet filtering is the prime mitigation mechanism for DDoS traffic because it guards against resource exhaustion in the network by preventing flooding. The probability for packet dropping reduces congestion across the network. Therefore, legitimate traffic flows freely, thus enhancing system performance during an attack.

**6.2.3.2 Performance on Network:**

The state of the network before, during, and after deploying the mitigation strategy was evaluated by tracking several performance metrics. These include:

Throughput: Before the attack, throughput was reliable in the network. The legitimate devices communicated properly. During the attack, the throughput drastically dropped due to network traffic congestion from DDoS traffic. However, once the packet filtering mechanism was activated, the throughput returned to normal levels, implying reduced malicious traffic.

Latency: Like throughput, latency surged dramatically during the DDoS attack because much traffic was introduced to the network to process. Once mitigation occurred, latency returned to normal since the filtering technique forced traffic back into the acceptable network congestion zone.


**6.3 Visualization of Results**

To explain in greater detail the GNN model's behaviour as well as the effectiveness of the mitigation strategy, we have used several visualization methods throughout the course of this project.


32

**6.3.1 Loss and Accuracy Graphs:**

The training procedure is followed by metrics tracking in terms of the loss and accuracy at each epoch. The graphs shown in the following images represent the learning process of the model. It is proved that the loss curve decreases because the model learns every detail of the data; this is reflected by the graph on accuracy that improves rapidly for the model in terms of its ability to classify objects.




**Fig. 6.1 GNN Model Training Accuracy Graph**



**Fig. 6.2 GNN Model Training Loss Graph**


33



**Fig. 6.3 Class Distribution Graph**

**6.3.2 Confusion Matrix:**

The confusion matrix will be represented to analyse how well the model distinguishes between benign and DDoS traffic, and the visualization may reveal patterns in false positives and negatives, helping identify regions where the model may need additional tuning.




**Fig. 6.4 Confusion Matrix**

34

**6.3.3 Network Animation:**

The NS3 simulation results came alive using the NetAnim tool, visualizing the network topology, the flow of traffic, and the impact of the applied mitigation strategy. Such animation enables us to visualize the whole interaction between nodes during the attack as well as how the patterns of traffic changed once packet filtering was applied. It also provides a perspective into how the nodes were distributed in space and the nature of the traffic movement between them, which is vital to understand the true effects of the mitigation strategy in real time.



**Fig. 6.5 Network Animation Simulation**

35

**CHAPTER 7**

**CONCLUSION AND FUTURE ENHANCEMENTS**

In this section, we present the results of the project and a roadmap for future improvements. Indeed, the approach from the project-a combination of AI-driven dynamic fuzz testing, GNNs, and a NS3-based simulator has proven to be quite promising for improving IoT networks, first and foremost in terms of security against DDoS attacks. However, in the field of IoT security, there is an evolution of challenges, and they present themselves every now and then. On this front as well, there is a need for a system to be in perpetuity improvement and adaptation. Finally, below, we summarize what we have found out and think some potential improvements that could make the system even more robust, scalable, and adaptive to real-world demands.

**7.1 Summary of Findings**

The novelty AI-driven fuzz testing methodology created dynamic traffic data on the NS3 network simulator. We produced a rich dataset consisting of benign traffic and DDoS attack traffic. We relied on fuzz testing to simulate some variability and predictability of the IoT environment, known for its heterogeneity, limited resources, and susceptibility to a broad range of attacks.

**7.1.1 AI-Driven Dynamic Fuzz Testing**

The module had used AI with Graph Neural Network (GNN) which was intended to identify malicious IoT network traffic patterns. It was understood that traditional learning algorithms would not work great in the case of graph-structured data and represented relationships among the IoT devices, which have thousands of interconnected elements. GNNs instead did very good discoveries of complex relationships and indirect dependencies where it mattered the most in graph-structured data and therefore best suited for IoT applications.

In our system, the GNN was trained on data outputted from the NS3 simulator, which provided it with a controlled testing environment for dynamic traffic scenarios. The model was trained in such a way that it achieved 74% validation accuracy, which is important considering the dynamic nature of IoT traffic. Although there is still room for improvement in this accuracy, it shows that the GNN can generalize well to unseen traffic patterns without overfitting. This validates the perception that there is a contradiction between the low validation accuracy and nearly perfect training accuracy because of the extreme differences in traffic behaviour; most of them are due to differences in devices, protocols, and network configurations.

36

**7.1.2 NS3 Simulation and Visualization**

The good simulation tool of powerful networking, NS3, was important to mimic real-world conditions of the IoT network. The simulator gave the needed infrastructure to test how well our system could detect and counter DDoS attacks in an environment close to the real world IoT traffic. Using NS3 gives us the chance to create profound patterns in the traffic to see and understand what is happening with malicious traffic, such as increased latency and decreased throughput, on a network.

We also used NetAnim, where we could see the dynamic flow of the traffic through the network in real-time. This is what, therefore, made the visual representation necessary for verification purposes in ascertaining if the strategy was working to curb the malicious transmissions because it provided evidence on how to spot and filter out such malicious traffic. If the GNN had detected an IP address, then NS3 was set to automatically drop all packets coming from that address. This packet-dropping mechanism has significantly reduced network congestion from DDoS traffic, and generally resulted in better overall performance.

**7.1.3 Countermeasures**

To mitigate the attack, the system will identify and drop packets coming from malicious IP addresses. This will successfully reduce the burden on the network, allowing genuine traffic to pass through. For IoT environments, for example, healthcare systems or smart cities, where network reliability is of paramount importance, failure in the network would have critical ramifications.

The packet-dropping mechanism appears to reveal some measurable improvements in network performance metrics. In a DDoS attack, the malicious packets drop served to significantly reduce network congestion and produced increases in throughput and latency correlated with this reduction. Such performance benefits provide evidence for the system's ability to ensure quality of the network despite the attack it may be under. The confusion matrix, a crucial method for measuring classification accuracy in the model, further revealed that the system can classify DDoS traffic with accuracy with minimal false positives and false negatives in the classification decision.

**7.2 Future Improvement**

Although the present system significantly Favors detecting and reducing the destructive nature of DDoS attacks in IoT networks, there are still many improvements that can be applied to further improve the overall performance, adaptability, and scalability factors. Some of the significant areas of improvement in the future are discussed below.

37

**7.2.1 Real-time Mitigation**

The real-time mitigation capability is one of the most important future development directions. Currently, a time lag exists between malicious traffic detection and incorporation of the strategy for mitigation. Such a delay may severely affect the timely delivery of certain IoT applications such as autonomous vehicles, smart grids, or healthcare systems. A brief network disruption in such applications could provoke catastrophic consequences.

To minimize this latency, the data pipeline of the system may be optimized to speed up the loop of detection to action. The use of edge computing methodologies will allow making decisions closer to the edge network on which the devices of the IoT are located. Since the processes of detection and mitigation can be decentralized, the detection and, hence, the subsequent mitigation could occur through edge devices in near real time too. This would further enhance its efficiency in delivering network performance during attacks.

**7.2.2 Elaborated Attack Scenarios**

Our system now protects against DDoS attacks; however, the IoT networks remain vulnerable to a myriad of cyberattacks including MITM attacks, SQL injection attacks, and data breaches. This definitely increases the utility and flexibility of the system exponentially through the extension into the detection and mitigation of other forms of attacks.

This will entail the design of more sophisticated datasets that capture the traffic patterns pertaining to a broader spectrum of attacks. The developed GNN model would be trained to recognize new patterns, thereby improving its capabilities with respect to a divergent set of threats associated with the IoT network. In addition, the modular architecture allowing for the realization of detection models for various types of attacks might make the system more flexible and adaptive towards new challenges associated with security.

**7.2.3 Scaling Test**

The scalability of an IoT network in a large-scale perspective is going to be one of the critical issues that are meant to be considered practically. All the testing that has been done so far has been within a controlled environment and with very limited devices. In real IoT networks, there might be thousands or millions of devices involved. This would cause a huge traffic, and thus the scalability along with heavy traffic performance needs to be tested in such a scenario for the system.

38

Future work might be implemented in distributed GNN implementations and the optimization of the packet filtering mechanism to provide effective and efficient operations of the system in high-throughput networks. Further improvement in scalability can also be made using distributed computing techniques such as parallel processing or federated learning in large IoT environments.

**7.2.4 Adaptive Learning**

Another improvement aspect is the adaptation of adaptive learning techniques. In the adaptive nature of an IoT environment, both network behaviour and attack patterns might change drastically. The static model, trained on a single dataset, may not be able to keep up with changes in those dynamics. Online learning techniques or reinforcement learning could be adapted so that the GNN model can keep learning over new data inputs and improve adaptability to changing network conditions. This would mean having detection levels accurate even with new emerging attack vectors in the system. It will also prevent overfitting since the model is going to refresh often with new data rather than sticking to old patterns.

**7.2.5 Integration of Security Tool**

The functionality of the current system can be improved highly. Thus, with integration into other security tools and frameworks, the system can detect and curb DDoS attacks effectively. For example, if the system is combined with IDS, firewalls, and SIEM systems, a more integrated security solution for IoT networks would be produced.

Such integration would, therefore, ensure an all-around approach to IoT security, with real-time monitoring, detection, and mitigation of a wide range of threats in cyber space. Such an integration would easily amalgamate with established infrastructures in real-world environments, providing end-to-end protection for IoT networks.

**7.3 Conclusion**

In conclusion, our dynamic fuzz testing technique based on Graph Neural Networks with simulations in NS3 has been promising as a key for enhancing the security of IoT environments. Here, the ability of the system to detect DDoS attacks with an accuracy of 74% generally indicates its potential utility in practical applications. In addition, the packet-dropping mitigation strategy has shown that it can enhance network performance by maintaining the throughput of the network and reducing the latency in the case of DDoS attacks.

39

The current system shall provide a good base. A couple of more advancements in the areas of real-time mitigation techniques, attack scenarios to check, scalability testing, adaptive learning, and integration with other security tools would make the system robust, adaptable, and scalable, having the potential for keeping up with the growing complexity and diversity of IoT networks.

Synthesizing advanced AI techniques with traditional network simulation tools presents an incredibly powerful approach toward addressing the challenges posed by security in IoT networks. As IoT networks grow in scale, our ability to protect them from growing sophistication in cyberattacks must keep pace. That is what this project represents in that direction, and the list of future enhancements detailed here paints a clear picture of what needs to be done to further build up the system in terms of effectiveness and resilience.

40

**REFERENCES**

1. M. Althobaiti and R. Alshammari, "IoT Security: Challenges and Potential Solutions," Journal of Cyber Security and Information Systems, vol. 1, pp. 45-60, 2023.
2. T. Nguyen and W. Li, "Man-in-the-Middle Attacks in IoT Networks: Vulnerabilities and Countermeasures," IEEE Internet of Things Journal, vol. 10, no. 1, pp. 88-98, 2023.
3. M. A. Khan and K. Salah, "IoT Device Security: Firmware Management and Patch Distribution," International Journal of Network Security, vol. 25, no. 2, pp. 101-115, 2022.
4. M. Aslan and R. Samet, "A Comprehensive Survey on DDoS Attacks and Countermeasures in IoT Networks," IEEE Communications Surveys & Tutorials, vol. 25, no. 3, pp. 1-30, 2023.
5. Y. Mirsky, I. D. Luchin, T. Avgerinos, and G. Oikonomou, "Anomaly Detection for DDoS Attacks in IoT Networks Using Machine Learning," IEEE Transactions on Network and Service Management, vol. 19, no. 1, pp. 112-125, 2022.
6. E. Alomari, M. Qatawneh, and A. Otoom, "DDoS-Resistant Protocols for IoT Networks: A Survey," IEEE Access, vol. 11, pp. 660-675, 2023.
7. W. Ali and F. Hussain, "Machine Learning-Based Security Frameworks for IoT Networks," IEEE Internet of Things Magazine, vol. 5, no. 4, pp. 100-110, 2022.
8. T. N. Kipf and M. Welling, "Graph Neural Networks for Network Security Applications," Journal of Network and Computer Applications, vol. 100, pp. 59-72, 2023.
9. X. Zhang, Y. Liu, Z. Li, and H. Wang, "GNN-based Anomaly Detection for Securing IoT Networks," IEEE Transactions on Information Forensics and Security, vol. 18, pp. 499-512, 2023.
10. M. Böhme, V. J. M. Arruda, and A. Zeller, "Dynamic Fuzz Testing for IoT Security," ACM Transactions on Privacy and Security, vol. 25, no. 2, pp. 88-105, 2022.
11. K. Lee, S. Lee, J. Kim, and C. Kim, "Integrating Fuzz Testing with AI for Enhanced IoT Security," IEEE Transactions on Dependable and Secure Computing, vol. 20, no. 4, pp. 1510-1520, 2023.

41

1. S. Wang, Y. Zhang, and L. Tan, "AI-Driven Dynamic Fuzz Testing in IoT Security: A Comprehensive Review," IEEE Transactions on Industrial Informatics, vol. 19, no. 5, pp. 660-675, 2023.
2. Ns3-dev Team, "NS3: A Simulation Tool for IoT Security Research," NS3 Documentation, 2023. [Online]. Available: https://www.nsnam.org/docs/. [Accessed: 26-Aug-2023].
3. Y. Zhu, L. Ma, and H. Xiao, "Simulating IoT Security Solutions Using NS3," Journal of Internet Services and Applications, vol. 14, no. 2, pp. 200-210, 2023.
4. S. Sharma and R. Gupta, "AI-Based Solutions for Securing IoT Networks: A Survey," Future Generation Computer Systems, vol. 152, pp. 88-102, 2023.
5. K. Patel, R. Roy, and S. K. Sharma, "Mitigating DDoS Attacks in IoT Using AI Techniques," IEEE Internet of Things Magazine, vol. 6, no. 2, pp. 110-121, 2023.
6. J. Thompson and A. Miller, "Graph Neural Networks for Cybersecurity: A Review," Journal of Cyber Security Technology, vol. 7, no. 3, pp. 225-240, 2022.
7. Y. Zhang, X. Wang, and T. Chen, "Advanced Fuzz Testing Techniques for Network Security," IEEE Transactions on Network and Service Management, vol. 20, no. 1, pp. 88-98, 2023.
8. P. Williams, T. Yang, and X. Hu, "Real-Time DDoS Detection in IoT Networks Using Machine Learning," IEEE Transactions on Information Forensics and Security, vol. 18, no. 1, pp. 123-134, 2023.
9. H. Liu, X. Chen, and Q. Zhang, "Enhancing IoT Security with AI-Based Approaches," IEEE Internet of Things Journal, vol. 9, no. 4, pp. 287-298, 2022.
10. C. Ozturk and M. Gunes, "A Comprehensive Survey on Network Security Simulation Tools," IEEE Communications Surveys & Tutorials, vol. 25, no. 2, pp. 60-90, 2023.
11. El-Sayed, M. Elhoseny, and M. Abdel-Badeeh, "A Deep Learning Approach to IoT Security Using GNNs," IEEE Transactions on Dependable and Secure Computing, vol. 19, no. 2, pp. 88-100, 2023.
12. R. Anderson, G. Brown, and L. Zhang, "Securing IoT Networks with Advanced Fuzz Testing," ACM Transactions on Privacy and Security, vol. 25, no. 3, pp. 112-130, 2022.

42

1. L. Tan, J. Qian, and M. Zhou, "AI-Driven Approaches for DDoS Mitigation in IoT Networks," IEEE Access, vol. 11, pp. 660-675, 2023.


43

**APPENDIX A**

**CONFERENCE**

**PRESENTATION**

Our paper titled "**AI-Driven Dynamic Fuzz Testing for IoT Security: Detection and Mitigation of DDoS Attacks Using Graph Neural Networks**" has been conditionally accepted for oral presentation in the 4th International Conference on Cognitive & Intelligent Computing (ICCIC), under the Networks, Privacy & Security track. The conference will be conducted in a hybrid mode on November 29-30, 2024. Our paper ID is 223, and we have a plagiarism score of 4%.




**Figure A.1: ICCIC 2024 Acceptance**

44

**APPENDIX B**

**PLAGIARISM REPORT**



45